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	Supplier:
	

	Order number:
	

	Position:
	

	Drawing number:
	



	No.
	Criteria
	Request
	Examination carried out

	1
	Structure and course
	Visually visible deviations (e.g. orange peel, brush strokes, roller prints, etc.) are not permitted.
	|_|

	2
	Visible material defects, rolling cracks, scars
	Not allowed
	|_|

	3
	Material scratches, burr formation, other damage
	Not allowed
	|_|

	4
	Spot weld marks
	Not allowed
	|_|

	5
	Bishop
	Not allowed
	|_|

	6
	Pinpricks, open pores
	Not allowed
	|_|

	7
	Blistering
	Not allowed
	|_|



Coating thickness measurement (dry film thickness)
The measuring points must be marked on the drawing and attached to this report.

	|_|   Wet painting 
	|_|   Powder coating



	Point
	Thickness
	Point
	Thickness
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